• |
Supermoto | XL
| Designs | •
"Turning Ideas into designs" | ( http://www.supermotoxl.com )
author: David L. (SupermotoXL) | e-mail: davidlimars@hotmail.com
• XYBORX ED 32.1 XL-XGT | Released Date: 27 April 2015
Read the information and instruction below before proceed with models editing, porting, conversion and other project. Be sure you understand all the information stated below. For more information, support and tools you can go to our website for updates and downloads.
Disclaimer: The contained files are provided "as is" without warranty of any kind, either expressed or implied. The author will not be held responsible for any losses incurred, either directly or indirectly by the use of these files.
• SupermotoXL Developer Kit (Original high resolution 3D models production set)
Welcome to SupermotoXL Developer Kit (Original model development kit). This page is the heart and original resources of my designs, the quality and originals is here where enthusiast modeler, game developer and avid add-on/game mods can grab/download some models in here for their various projects. Here are some of the uncompiled models which i've previously designed now available for public usage. If you need to find perfect models for your project, model editing, game add-on porting, conversion, animation or just modding for showcase then this is the right place for you to download raws of high quality models. Each models are perfectly built and ready to be ported into any games genre or simply for having fun.
The content attached with this package contain 3d meshes, texture and support file that only to be use for 3d models development, modification and editing purposes. Enjoy.
• General Information
Model name | - | XYBORX ED 32.1 XL-XGT
Original release | - | Racing simulation / Second Life
Release date | - | 27-4-2015
Vehicle name | - | XYBORX ED 32.1 XL-XGT
• Production details
Model version | - | 32.1
Prod. No | - | 20042015
Brand/Manufacturer | - | SupermotoXL
Model type | - | Super car
• Models Specification
Category | - | SupermotoXL Developer Kit (Original high resolution 3D models production set)
Original format | - | "xyborx_cd321xlxgt.z3d" Z3d (Z-modeler)
Optional format | - | -
Avg face count | - | 119989
Avg vertices count | - | 127622
(unit) x max texture size | - | (1x) 4096x4096 "xby32xgt.tga" (model body texture)
(unit) x min texture size | - | (1x) 512x512 "*wh_rvxf6xl.tga" (wheel texture) + (1x) 1024x1024 "xb_floor.tga" (floor texture)
Reflection texture size | - | (2x) 256x256 "chrome.bmp" (reflection texture)
Optional alpha filter | - | No
Optional parts | - | no
Transparency parts | - | yes
Reflection support | - | yes
Showcase ready | - | yes (simple stage floor)
approx uncompress file size | - | 60.0 MB
Recommended 3d editing tools | - | Z-modeler
• Texture theme included
Themed texture pack | - | xby32xgt.tga (Default -Original)
• Production tools
3D program | - | Z-modeler 1.07
Optional format | - | Corel Photopaint
• Released History / Previous version feedback
Target platform/game | - | PC
Parent model & variant | - | XYBORX ED 32.0 XL-RL
Format | - | Z3D "Z-modeler" format (xyborx_cd321xlxgt.z3d)
Quality grade | - | 4096 HD
Distribution restriction | - | Free/Open public
Source | - | http://www.supermotoxl.com
- | - |
The XGT is the car for those who like a classic retro racer yet with modern touch. It has the chromes, the blink, muscle bulges, classic retro curve, long big block V12 engine, kung Fu 'Bruce Lee' style era theme, shiny drag racing billet rims, carbons upgrades, radical down force spoiler and masculine car for manly man. The only car you can drive like a boss and doesn't age through time. The XGT variant have slightly increase horsepower than stock engine and CC size. Due to lighter bodyweight it has better launch speed acceleration and short distance stopping power. Unlike the 'RL' stock model 'XGT uses XLE11 generation engine that has more torque and rpm. Other addition feature added into 'XGT' is differential lock mechanism which allow full differential lock either in 4WD or 2WD to allow 100% full torque transmission to all 2-4 wheels during straight line acceleration/drag racing performance. INTRODUCTION (Same as parent model 'RL') ________________________________________________________________________________________ XYBORX is an evolution from the first generation CYBORX from the year 2005. The first generation was the stepping stone for SupermotoXL Designs to start a new fresh ideas of unique supercars which lead to todays lines of SupermotoXL's models. 6 years later I decided its time to show what new generation XYBORX is all about. The new XYBORX carry attributes of both muscle and exotic import looks and feel giving best impression to various motor fans on both worlds. Originally XYBORX was "backdoor" launched on mid 2013 for beta tester without internal cockpit...in fact i'm not all good designing interior cockpit so i left that one behind. First used on EVO2 for test drive then ported by other into other game such as GTA for unofficially to test polycount lag (FPS performance). The first releases didn't get much publicity because i didn't have time and resources to spent much on 3D design and gaming development. 2011-2013 was a bad year for me to public launched it due to time constraint and career thing. Then i was all out into real world activity leaving backdoor tester to do their open work and mods and almost forgot all about it. 2 years later after done pursuing other goals such as 3d Printing tech, R/C models and FPV/UAV flight development i've return to work on XYBORX for its final release after receiving few feed back from past backend user. Although the car by now is an ancient relic after years of abandonment in the dust it still was most long awaited car by fans who have rooted by first generation CYBORX most popularly used in gaming and social virtual world such as GTA and SECOND LIFE. The car itself still looks 'badass' in its own term and ought to have a place in virtual motoring world. THE DESIGN (Same parent model 'RL') ________________________________________________________________________________________ XYBORX intended to replace the old 1st generation CYBORX which is by now on 2015 its already 10 years old but already had many fans all over the globe via virtual motor racing. The new XYBORX uses base chassis from CONXERTO morphed longer wheel base with muscular Hemispheric (HEMI) big block V12 engine mounted forward under the front hood which is why the font chassis are longer than any car i designed. XYBORX new body design and looks was aim to have both a classic muscle car feeling and a touch contour of an exotic import super car, so i bulk up each curve on its outline have a muscular looks especially around the wheel fender body works and hatch back like imports rear appearance with a streamline frontend looks of a modern street racer. Just like other SUPERMOTOXL's generation of exotic design the headlights re-designed to show how it has evolve though time with more unique stream lined of fins integrated with engine vents all the way to the lower side of wheel fender, Integrated headlight and side vented. The left and right headlight fin that grooved from front to the rear side have air intake duct integrated into headlight fins serve as engine carburetor and air coolant dually both left and right side of the hood event though existing ones included in the middle of the hood. Heat from the engine escape from the side vents before the door panel. Long classic muscle dragster body One most notable striking looks of the new XYBORX compare to all of my designs was a very long chassis design with long wheel base. Not only just to accommodate long inline Hemispheric V12 engine (XLE11-X12HH) but also to keep the car run stable at straight line without problem swerving around. Bigger front chassis not only to accommodate bigger engine but also helps to trap in more air into the engine via big and multiple ventilation from the front end to cool the engine and also to generate air hydraulic kinetic to power overall operation inside car. Surplus of air escape from side vent before the door and another air channel to the rear center duct to generate down force to keep the car rooted on the ground via Bernoulli effect. In addition to the drag design the stock tires are thicker and bigger profile for better drag racing grip in all corner. Brushed stainless steel out body Like NEMXIS XGT, the outer body shell of XYBORX are made out of brushed stainless steel finishing to give a exotic luxury looks. Unfortunately it doesn't use Composite Lexan OPLEC (Organic Passive Light Emitting Cell) shell like previous car do due in favor of exotic steel luxury 'bling' factor for XYBORX. Other cool new creative innovation applied to this car other than ventilated headlights is a pair of 'Jack-up' doors. 'Jack-up' open vertically straight 45 degree up parallel to the chassis to allow maximum passenger exist clearance...plus it looks cool. TECHNOLOGY (Same parent model 'RL' but with XLE11* engine) ________________________________________________________________________________________ Other special feature built in XYBORX which also similarly applied to previous models includes: OHID headlights and OCDLED rear lights "integrated vent fins" : OHID (Organic Hi-Density headlights) and OHLED (Organic Controlled Density LED rear lights) is a new technology which uses flexible and low charged high luminance thin light panel made from organic cell structure (cob webbed cells). These panel are shock resistant and consume low electric current yet it produce high output of light just similarly used on LCD and Plasma panel. Multi-channel Bernoulli Ventilation System: Just like its brother XAVAGE and CONXERTO, XYBORX have built in “Air Buoyancy Chassis” which allow air to circulate full 360 degree range around the chassis for few cycle before exit out to rear end air exhaust port. This feature helps to cool the chassis and components in the car and also allow natural hydraulic cushion. The Multi-Channel Bernoulli Ventilation System which located 2x on the front to gulp massive air by force into the chassis and tunnel the air into several channel for above purpose. Other than “Air Buoyancy” feature other use of tunneled air includes auto deflation control of tire pressure, suspension shock pressure, engine turbo compression, pneumatic pressure discharge, force combustion discharge, inner down-force system between wheels, power regeneration via air turbine for power charging, air pressure refill for hybrid engine module for kinetic propulsion, artificial cockpit, engine coolant coolant and pressure balance between inner and outer body wall. XLE11-X12HH Engine for XGT: XYBORX XGT uses semi enhanced hybrid fused into Hemispheric engine technology that runs 60% propulsion from fossil fuel energy and 50% electric under single engine block yet modular in mechanism. Fuel powered module: As usual XYBORX share same “X12” engine spec as her parents the CONXERTO, XAVAGE, NEMIXIS and X3-SIXTY where piston configuration remain in “X” push layout for complete 360 degree equal torque for every drive shaft turns per- revolution. 4 lines of piston in partitioned in to 4 in every 360-degree distribution where each lines have each line consist of 3 piston (3 piston x 4 lines) = 12 piston. These configuration taking advantages over standard “V” overhead engine, Boxter engine horizontal push and Rotary engine layout. “X12” allow high acceleration and lower fuel injection to combust per-joule, But the difference in XYBORX is it has bigger block to accommodate bigger hemispheric header for extra 10% bigger combustion that previous engine model. Electric module: Consist of twin brushless motor powered by high capacity rechargeable lithium ferum (Li-Fe) battery. The motor controlled by computer programmed ESC (Electronic Speed Controller) to propel the motor according to required rpm. The motor connected to variable ratio gear case and then interfaced to main engine’s main 1 way turn spur gear. As the spur gear turned by electric powered brushless motor the spur will auto disengage from fuel powered engine drive crank shaft to reduce mechanical load from the engine, which the electric powered system will take over the full transmission drives. Kinectic module: Kinetic module is a mechanism, which is powered by stored energy produced by kinetic output such as air pressure and heat source. XYBORX carries 2x150 liters of air tank which store compressed air collected from various vents around its chassis. These air tanks located under the rear hatch back. Each tanks can handle 80 bars of barometric air pressure, Collected air will be used as air compression source to push turn and propels 4x turbo-turbine units on X12 fuel engine, 2x turbine pinion gear on both electric motors and 1x twin turbine built-in main spur gear. To summarize that the air are mainly to boost all the cycle of the gear reducing the burden of acceleration thus save both fuel and electric cell. The heat kinetic are used to heat up the tank thus increasing the pressure of the air before gush into output mechanism. The heat source comes from fuel engine, electric motor and external environment via Radiator system. GYRO system: XYBORX is equipped with 6x axis MEMs GYRO system which allow the car to run stable during speeding, drift and cornering. The gyro components links to several components in the car to control the overall stability which includes: Front and rear differential Control the differential slips among 4 wheels by distribution proper traction needed during cornering, drift and an event when traction error and body instability detected. Note that XYBORX have 2WD to 4WD manual switching transmission. Steering Partially control the steering at micro level where as if GYRO needed to recover the car to proper lines if the driver swerve too much on the steering especially in wet condition and loose gripped surface such as sand, dirt, muddy trails and road full patches of holes. However in situation where the driver (dominant) control the steering the Gyro effort are only to control under steer and over steer error where it will try to synchronized the differential slips with the driver steering style to minimized stability error. ABS GYRO level of control is very much similar to “driver steering” detection protocol as mentioned before on steer part If any anomalies detected such as under steer/over steer braking or side ways braking the GYRO will engage ABS control plus will also control other components in the car which links to GYRO to synchronized with ABS system demand. The GYRO however does not cater 100% desirable handling as driver wanted, it can actually be enabled and disabled manually by the driver. When GYRO is active it offer several option where the driver can select according to his or her driving preferences, these are: Cruise/Normal mode (default): For normal car handling. Expert Touring/Racing mode: Racing and high speed touring handling. Drift mode: Drift handling. More differential gear control involve. Drag mode: Straight line handling with high anti-sideway control. Very heavy use of down force mechanism. Front and rear differential lock capability: Allow full 100% non-slip transmission drive to all wheel optimized for straight line drag racing. Off-road: For off-road handling. Preset/Learning mode: GYRO in learning mode (no control), feed and learning from drivers output, allow personalized handling from different driver’s style of handling. When Learning mode is completed the GYRO will cater several familiar handling mode to specific or assigned driver. FAIL SAFE mode: However if GYRO fail to function due to unknown distortion, damages or other accident which cause Gyro to shutdown a fail safe mechanism will be activated automatically and independently via mechanical system. The fail safe mode will reset all the configuration inside the car including differential, braking, engine, steering, suspension, hydraulic aerofoil and others back to normal mode without causing problem in driving ability. PERFORMANCE STATISTIC _______________________________________________________________
Specification for XYBORX "XGT" variant:
Max power | 3,920hp / 8700rpm |  | Max torque | 2,827.31ft-lb / 6520rpm
Engine | Semi Hybrid X-12H (XLE11-12HH/HEMI) |  | Displacement | 12080cc
Drive train | 2WD + 4WD + manual switch with differential lock capability. |  | Weight | 790kg
0-100km | 1.8 sec |  | Max Speed | 930kmh
0-300km | 6.9 sec |  | Braking (100-0km) | 29.5m / 2.3sec
_______________________________________________________________ SUMMARY about 'XGT' variant ________________________________________________________________________________________ The 'XGT' define what brute adrenaline car is all about. Two words: MUSCULINE and CLASSIC. Its the reason i got this far to build my dream car that is not only appealing but also has powerful message to convey to all motoring fans what real modern muscle car would look like and keep the legacy of classic muscle car DNA intact into modern world. I used to be a big fan of exotic Italian supercars with with modern curves and aerodynamic surfaces but after too seeing bunch of them in the market roaming around in useless body works i decided step into other side of roaring classic muscular car class based from the 70's muscle cars like old FORD MUSTANG, DE TOMASO PANTERA, FORD/SHELBY AC COBRA, Starsky & Hutch GRAN TORINO. ASTON MARTIN DB6 and 1967 TOYOTA 2000GT which inspire me to mix match classic design and incorporated into modern day looks...and also added some SUPERMOTOXL's DNA...the results XYBORX 'XGT'. In every angle view and corner you see on XYBORX ED 32.1 XL-XGT is all about beefy muscles, long body and low slung chassis, hatchback, sinister headlights, thick dragster tyres, sexy disc brakes, chromes and other attributes which was once proud as a classic entity from good old days of roaring carburetor engine. Mostly like the XYBORX XGT chassis will be used as future based chassis design for second generation EXODUS and EXAGE. We'll see how its goes. Till then enjoy the ride.
• |
Supermoto | XL
| Designs | •
"Turning ideas into design"
Enjoy.
Important note : 3d models checklist and notes
Please read the note below regarding the 3d meshes and texture issue.
In this SDK package include several material that should attached along together with this file these are:
1. | *.Z3D file (Z-modeler format)
2. | *.TGA file (Multiple of hi-resolution texture set)
3. | Sample of images file, 3d screenshots of actual models and image screenshot and details from 4x4evo1 and 4x4evo2 realtime in-game simulation.
| Before you start make sure you have proper 3d program/modeler tools. I recommend you to download Z-modeler v1.07 or Z-modeler v2 to open and edit *.Z3D file. You can download it at http://www.zmodeler2.com But if you already own a 3D Studio tools then you can open the existing *.3DS file attached in this package. But for high compatibility when viewing this models i recommend Z-modeler.
| By default these 3d meshes/models as usual runs perfect when editing using Z-MODELER tools because it was built using this tools from scratch, *.Z3D extension format is default Z-MODELER file. Before you open the *.Z3D file into Z-modeler program make sure the all *.TGA texture file located in the same location/directory where *.Z3D file is located else you'll have blank white meshes/models upon opening in Z-modeler.
| Make sure you double check if your Z-modeler or your 3D Studio program render the models as similar and as accurate as shown/published inside the models screenshots/images attached with this package. Make sure the reflection effect, transparency and parts are perfectly exhibited/shown correctly on your 3d tools view port. Good Luck.
• notice: LEGAL USAGE
You may freely use, edit , distribute, convert, host over the internet and other appropriate use for non-commercial purpose provided you should put/attached credits, details and links to the original author. For latest information, rules or article related on obtaining approval/permission please do visit our website at http://www.supermotoxl.com. You can also e-mail me at davidlimars@hotmail.com . Should you need to use it for commercial purpose please seek permission from me legally.
Should you require further information, please do not hesitate to contact me. E-mail: davidlimars@hotmail.com
* For more information on our latest designs, news, updates, services and other resources please visit my site at http://www.supermotoxl.com
• SupermotoXL Designs •
________________________________________________________________________________